COMM RESET statement

Purpose | Disable flow control for a given serial port.
Syntax | COMM RESET [#] hComm, FLOW
Remarks | Switches off all flow control to the serial port as specified by the file number stored in hComm. The Number symbol (#) prefix is optional, but recommended for the purposes of clarity.
See also | Serial Communications, COMM CLOSE, COMM function, COMM LINE, COMM OPEN, COMM PRINT, COMM RECV, COMM SEND, COMM SET, COMM TIMEOUT