Error 488 - Numeric processor overflow

Numeric processor overflow - Execution of this line of source code is complex, and requires more floating point registers than are currently available in the FPU. One solution might be to add the metastatement #REGISTER NONE to the current procedure, if register variables are being allocated. Another solution would be to break up the source code into multiple simpler statements.