TCP ACCEPT statement

Purpose | Accept an incoming request for communication from a specified TCP/IP port.
Syntax | TCP ACCEPT [#] fNum& AS newfNum&
Remarks | Accept an incoming connection request to the fNum& socket, and create a newfNum& socket handle to communicate with the new connection. TCP ACCEPT is only valid with sockets opened using TCP OPEN SERVER.
See also | TCP and UDP communications, TCP CLOSE, TCP LINE INPUT, TCP NOTIFY, TCP OPEN, TCP PRINT, TCP RECV, TCP SEND, UDP OPEN