Misc Operations

ASM | Identify an assembly-language statement.
ASM ALIGN | Rounds up the instruction location to a power of two address
ASMDATA/END ASMDATA | Define a block where primitive read-only data is stored.
BEEP | Play the default Windows sound through the computer speaker(s).
IMPORT | Load or free a library ( DLL) to access an imported procedure.
PLAY WAVE | Play a sound under program control.
PLAY WAVE END | Stops any waveform sound which is currently playing.
REM | Indicates the remainder of a line of source code is a remark or comment.