; OEMSETUP FILE FOR Intel 2104x/2114x 10/100 mbps Ethernet Controller , v5.02
;     NDIS 4.0  - Windows NT 4.0 -
;
;     Supported adapters:
;           Intel 21040 based Ethernet Controller
;           Intel 21041 based Ethernet Controller
;           Intel 21140 based 10/100 mpbs Ethernet Controller
;           Intel 21142 based 10/100 mbps Ethernet Controller
;           Intel 21143 based 10/100 mbps Ethernet Controller
;           Intel EB40 21040 based Evaluation board
;           Intel EB41 21041 based Evaluation board
;           Intel EB140 21140 based 10/100 mpbs Evaluation board
;           Intel EB142 21142 based 10/100 mpbs Evaluation board
;           Intel EB143 21143 based 10/100 mpbs Evaluation board
;           DEC multia's Ethernet Controller
;           DEC DE434 PCI Ethernet Adapter
;           DEC DE435 PCI Ethernet Adapter
;           DEC DE450 PCI Ethernet Adapter
;           DEC DE500 PCI Fast Ethernet Adapter
;           DEC DE425 EISA Ethernet Adapter
;
; Intel Corporation 1998
;
; Usage:
;
;     This file is the installation/configuration/deinstallation
;     procedure of the Intel DC21x4 driver for Windows NT.  It can be called
;     from Windows Setup directly, or via the Windows NT Networks
;     Control Program Applet (NCPA) from inside the Windows
;     Control Panel.
;
;----------------------------------------------------------------------------------------
[Identification]
    OptionType = NetAdapter
[PlatformsSupported]
    ISA
    EISA
    "Jazz-Internal Bus"
    PCI
[Options]
    DC21040
    DC21041
    DC21140
    DC21142
    DC21143
    EB40
    EB41
    EB140
    EB142
    EB143
    E143DQS
    MULTIA
    DE434
    DE435
    DE450
    DE500
    DE425
[ConnectionChoicesDC21040]
    Connect_0 = "AutoDetect", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full Duplex ", 3
    Connect_3 = "10BaseT (TP) No_Link_Test", 4
    Connect_4 = "10Base2 (BNC)", 1
    Connect_5 = "10Base5 (AUI)", 5
[ConnectionChoicesDC21041]
    Connect_0 = "AutoSense", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full Duplex ", 3
    Connect_3 = "10BaseT (TP) No_Link_Test", 4
    Connect_4 = "10Base2 (BNC)", 1
    Connect_5 = "10Base5 (AUI)", 5
[ConnectionChoicesDC21140]
    Connect_0 = "AutoSense", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full Duplex ", 3
    Connect_3 = "100BaseTx (TP 100)", 8
    Connect_4 = "100BaseTx (TP 100) Full Duplex", 9
    Connect_5 = "100BaseT4", 10
    Connect_6 = "100BaseFx", 11
    Connect_7 = "100BaseFx Full_Duplex", 12
[ConnectionChoicesDC21142]
    Connect_0 = "AutoSense", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full Duplex ", 3
    Connect_3 = "10BaseT (TP) No_Link_Test", 4
    Connect_4 = "10Base2 (BNC)", 1
    Connect_5 = "10Base5 (AUI)", 5
    Connect_6 = "100BaseTx (TP 100)", 8
    Connect_7 = "100BaseTx (TP 100) Full Duplex", 9
    Connect_8 = "100BaseT4", 10
    Connect_9 = "100BaseFx", 11
    Connect_10 = "100BaseFx Full_Duplex", 12
[ConnectionChoicesDC21143]
    Connect_0 = "AutoSense", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full Duplex ", 3
    Connect_3 = "10BaseT (TP) No_Link_Test", 4
    Connect_4 = "10Base2 (BNC)", 1
    Connect_5 = "10Base5 (AUI)", 5
    Connect_6 = "100BaseTx (TP 100)", 8
    Connect_7 = "100BaseTx (TP 100) Full Duplex", 9
    Connect_8 = "100BaseT4", 10
    Connect_9 = "100BaseFx", 11
    Connect_10 = "100BaseFx Full_Duplex", 12
[ConnectionChoicesEB40]
    Connect_0 = "10BaseT (TP) ", 2
    Connect_1 = "10BaseT (TP) Full Duplex ", 3
    Connect_2 = "10BaseT (TP) No_Link_Test", 4
[ConnectionChoicesEB41]
    Connect_0 = "AutoSense", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full_Duplex ", 3
    Connect_3 = "10BaseT (TP) No_Link_Test", 4
    Connect_4 = "10Base2 (BNC)", 1
    Connect_5 = "10Base5 (AUI)", 5
[ConnectionChoicesEB140]
    Connect_0 = "AutoSense", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full Duplex ", 3
    Connect_3 = "100BaseTx (TP 100)", 8
    Connect_4 = "100BaseTx (TP 100) Full Duplex", 9
[ConnectionChoicesEB142]
    Connect_0 = "AutoSense", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full Duplex ", 3
    Connect_3 = "10BaseT (TP) No_Link_Test", 4
    Connect_4 = "10Base2 (BNC)", 1
    Connect_6 = "100BaseTx (TP 100)", 8
    Connect_7 = "100BaseTx (TP 100) Full Duplex", 9
    Connect_8 = "100BaseT4", 10
    Connect_9 = "100BaseFx", 11
    Connect_10 = "100BaseFx Full_Duplex", 12
[ConnectionChoicesEB143]
    Connect_0 = "AutoSense", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full Duplex ", 3
    Connect_3 = "10BaseT (TP) No_Link_Test", 4
    Connect_4 = "10Base2 (BNC)", 1
    Connect_6 = "100BaseTx (TP 100)", 8
    Connect_7 = "100BaseTx (TP 100) Full Duplex", 9
    Connect_8 = "100BaseT4", 10
    Connect_9 = "100BaseFx", 11
    Connect_10 = "100BaseFx Full_Duplex", 12
[ConnectionChoicesE143DQS]
    Connect_0 = "AutoSense", 0
    Connect_1 = "10BaseT (TP) ", 2
    Connect_2 = "10BaseT (TP) Full Duplex ", 3
    Connect_6 = "100BaseTx (TP 100)", 8
    Connect_7 = "100BaseTx (TP 100) Full Duplex", 9
[ConnectionChoicesMULTIA]
    Connect_0 = "AutoDetect", 0
    Connect_1 = "10BaseT (Twisted_Pair) ", 2
    Connect_2 = "10BaseT Full_Duplex ", 3
    Connect_3 = "10BaseT No_Link_Test", 4
    Connect_4 = "10Base2 (BNC)", 1
    Connect_5 = "10Base5 (AUI)", 5
[ConnectionChoicesDE434]
    Connect_0 = "10BaseT (Twisted_Pair) ", 2
    Connect_1 = "10BaseT Full_Duplex ", 3
    Connect_2 = "10BaseT No_Link_Test", 4
[ConnectionChoicesDE435]
    Connect_0 = "AutoDetect", 0
    Connect_1 = "10BaseT (Twisted_Pair) ", 2
    Connect_2 = "10BaseT Full_Duplex ", 3
    Connect_3 = "10BaseT No_Link_Test", 4
    Connect_4 = "10Base2 (BNC)", 1
    Connect_5 = "10Base5 (AUI)", 5
[ConnectionChoicesDE450]
    Connect_0 = "AutoSense", 0
    Connect_2 = "10BaseT (Twisted_Pair) ", 2
    Connect_3 = "10BaseT Full_Duplex ", 3
    Connect_4 = "10BaseT No_Link_Test", 4
    Connect_5 = "10Base2 (BNC)", 1
    Connect_6 = "10Base5 (AUI)", 5
[ConnectionChoicesDE500]
    Connect_0 = "AutoSense", 0
    Connect_1 = "100BaseTx", 8
    Connect_2 = "100BaseTx Full_Duplex", 9
    Connect_3 = "10BaseT", 2
    Connect_4 = "10BaseT Full_Duplex", 3
[FileConstants]
UtilityInf      = "UTILITY.INF"
subroutineinf   = "SUBROUTN.INF"
SoftwareType    = "driver"
Exit_Code       = 0
NetEventDLL     = "%SystemRoot%\System32\netevent.dll"
IoLogMsgDLL     = "%SystemRoot%\System32\IoLogMsg.dll"
Manufacturer    = "Intel"
ProductMajorVersion     = "5"
ProductMinorVersion     = "03"
ProductVersion  = $(ProductMajorVersion)"."$(ProductMinorVersion)

VendorID = 4113  ;; 1011 (DEC)

;;for systemsoft cardwizard
PCMCIADBKeyName = $(!NTN_ServiceBase)"\Pcmcia\DataBase"
PCMCIARMKeyName = $(!NTN_ServiceBase)"\resman\MacDataBase"
PCMCIARMPKeyName = $(!NTN_ServiceBase)"\resman"
DC21X4Manufacture = "Intel"
DC21X4Model = "EB143CS - CardBus evaluation board"

ProductSoftwareName     = "DC21X4"
ProductSoftwareTitle    = "Intel DC21X4 Adapter Driver"
ProductSoftwareImagePath = "\SystemRoot\System32\drivers\DC21X4.sys"
NetRuleSoftwareType     = "DC21X4Sys ndisDriver DC21X4Driver"
NetRuleSoftwareUse        = $(SoftwareType)
NetRuleSoftwareBindForm = """DC21X4Sys"" yes no container"
NetRuleSoftwareClass    = {"DC21X4Driver basic"}
NetRuleSoftwareSWBindable = {"DC21X4Driver DC21040Adapter non exclusive 100",+
                             "DC21X4Driver DC21041Adapter non exclusive 100",+
                             "DC21X4Driver DC21140Adapter non exclusive 100",+
                             "DC21X4Driver DC21142Adapter non exclusive 100",+
                             "DC21X4Driver DC21143Adapter non exclusive 100",+
                             "DC21X4Driver EB40Adapter non exclusive 100",+
                             "DC21X4Driver EB41Adapter non exclusive 100",+
                             "DC21X4Driver EB140Adapter non exclusive 100",+
                             "DC21X4Driver EB142Adapter non exclusive 100",+
                             "DC21X4Driver EB143Adapter non exclusive 100",+
                             "DC21X4Driver E143DQSAdapter non exclusive 100",+
                             "DC21X4Driver MULTIAAdapter non exclusive 100",+
                             "DC21X4Driver DE434Adapter non exclusive 100",+
                             "DC21X4Driver DE435Adapter non exclusive 100",+
                             "DC21X4Driver DE500Adapter non exclusive 100",+
                             "DC21X4Driver DE450Adapter non exclusive 100",+
                             "DC21X4Driver DE425Adapter non exclusive 100"}

OptionHelpFile = "DC21X4.hlp"
ProductHardwareName = "DC21X4"

ProductHardwareDC21040Title = "Intel 21040 based Ethernet Controller"
NetRuleHardwareDC21040Type  = "DC21040 DC21040Adapter"
NetRuleHardwareDC21040Class = {"DC21040Adapter basic"}
AdapterDC21040Type = 5  ;; PCI board
HelpDC21040Id = 10
DC21040CFID = 135185    ;; 0x00021011

ProductHardwareDC21041Title = "Intel 21041 based Ethernet Controller"
NetRuleHardwareDC21041Type  = "DC21041 DC21041Adapter"
NetRuleHardwareDC21041Class = {"DC21041Adapter basic"}
AdapterDC21041Type = 5  ;; PCI board
HelpDC21041Id = 20
DC21041CFID = 1314833    ;; 0x00141011

ProductHardwareDC21140Title = "Intel 21140 based 10/100 mpbs Ethernet Controller"
NetRuleHardwareDC21140Type  = "DC21140 DC21140Adapter"
NetRuleHardwareDC21140Class = {"DC21140Adapter basic"}
AdapterDC21140Type = 5   ;; PCI board
HelpDC21140Id = 30
DC21140CFID = 593937     ;; 0x00091011
StoreAndForward = 0      ;; Store_and_forward mode disabled
TxmThreshold100 = 512    ;; 100Mbps default threshold

ProductHardwareDC21142Title = "Intel 21142 based 10/100 mpbs Ethernet Controller"
NetRuleHardwareDC21142Type  = "DC21142 DC21142Adapter"
NetRuleHardwareDC21142Class = {"DC21142Adapter basic"}
AdapterDC21142Type = 5   ;; PCI board
HelpDC21142Id = 40
DC21142CFID = 1642513   ;; 0x00191011
ProductHardwareDC21143Title = "Intel 21143 based 10/100 mpbs Ethernet Controller"
NetRuleHardwareDC21143Type  = "DC21143 DC21143Adapter"
NetRuleHardwareDC21143Class = {"DC21143Adapter basic"}
AdapterDC21143Type = 5   ;; PCI board
HelpDC21143Id = 50
DC21143CFID = 1642513   ;; 0x00191011


ProductHardwareEB40Title    = "Intel EB40 21040 based Evaluation board"
NetRuleHardwareEB40Type     = "EB40 EB40Adapter"
NetRuleHardwareEB40Class    = {"EB40Adapter basic"}
AdapterEB40Type    = 5  ;; PCI board
HelpEB40Id = 100
EB40CFID = 135185         ;; 0x00021011

ProductHardwareEB41Title    = "Intel EB41 21041 based Evaluation board"
NetRuleHardwareEB41Type     = "EB41 EB41Adapter"
NetRuleHardwareEB41Class    = {"EB41Adapter basic"}
AdapterEB41Type    = 5  ;; PCI board
HelpEB41Id = 110
EB41CFID = 1314833        ;; 0x00141011

ProductHardwareEB140Title    = "Intel EB140 21140 based 10/100 mpbs Evaluation board"
NetRuleHardwareEB140Type     = "EB140 EB140Adapter"
NetRuleHardwareEB140Class    = {"EB140Adapter basic"}
AdapterEB140Type    = 5  ;; PCI board
HelpEB140Id = 120
EB140CFID = 593937         ;; 0x00091011

ProductHardwareEB142Title = "Intel EB142 21142 based 10/100 mpbs Evaluation board"
NetRuleHardwareEB142Type  = "EB142 EB142Adapter"
NetRuleHardwareEB142Class = {"EB142Adapter basic"}
AdapterEB142Type = 5   ;; PCI board
HelpEB142Id = 130
EB142CFID = 1642513    ;; 0x00191011


ProductHardwareEB143Title = "Intel EB143 21143 based 10/100 mpbs Evaluation board"
NetRuleHardwareEB143Type  = "EB143 EB143Adapter"
NetRuleHardwareEB143Class = {"EB143Adapter basic"}
AdapterEB143Type = 5   ;; PCI board
HelpEB143Id = 140
EB143CFID = 1642513    ;; 0x00191011

ProductHardwareE143DQSTitle = "Intel EB143DQS-20 21143 based 10/100 mpbs only Evaluation board"
NetRuleHardwareE143DQSType  = "EB143 EB143Adapter"
NetRuleHardwareE143DQSClass = {"EB143Adapter basic"}
AdapterE143DQSType = 5   ;; PCI board
HelpE143DQSId = 140
E143DQSCFID = 1642513    ;; 0x00191011


ProductHardwareMULTIATitle = "DEC multia's Ethernet Controller"
NetRuleHardwareMULTIAType  = "MULTIA MULTIAAdapter"
NetRuleHardwareMULTIAClass = {"MULTIAAdapter basic"}
AdapterMULTIAType = 5  ;; PCI board
HelpMULTIAId = 200
MULTIACFID = 135185    ;; 0x00021011
SiaRegister0 = 12353   ;; CSR13 = 0x3041
SiaRegister1 = 0         ;; CSR14 = 0x0000
SiaRegister2 = 6         ;; CSR15 = 0x0006

ProductHardwareDE434Title   = "DEC DE434 EtherWORKS Turbo PCI TP Adapter"
NetRuleHardwareDE434Type    = "DE434 DE434Adapter"
NetRuleHardwareDE434Class   = {"DE434Adapter basic"}
AdapterDE434Type   = 5  ;; PCI board
HelpDE434Id = 210
DE434CFID = 135185        ;; 0x00021011

ProductHardwareDE435Title   = "DEC DE435 EtherWORKS Turbo PCI Combo Adapter"
NetRuleHardwareDE435Type    = "DE435 DE435Adapter"
NetRuleHardwareDE435Class   = {"DE435Adapter basic"}
AdapterDE435Type   = 5  ;; PCI board
HelpDE435Id = 220
DE435CFID = 135185        ;; 0x00021011


ProductHardwareDE450Title    = "DEC DE450 EtherWORKS Turbo PCI Combo Adapter"
NetRuleHardwareDE450Type     = "DE450 DE450Adapter"
NetRuleHardwareDE450Class    = {"DE450Adapter basic"}
AdapterDE$50Type    = 5  ;; PCI board
HelpDE450Id = 240
DE450CFID = 1314833        ;; 0x00141011

ProductHardwareDE500Title   = "DEC DE500 FastEtherWORKS 10/100 PCI Adapter"
NetRuleHardwareDE500Type    = "DE500 DE500Adapter"
NetRuleHardwareDE500Class   = {"DE500Adapter basic"}
AdapterDE500Type   = 5  ;; PCI board
HelpDE500Id = 250
DE500CFID = 593937     ;; 0x00091011

ProductHardwareDE425Title   = "DEC DE425 EISA Ethernet Adapter"
NetRuleHardwareDE425Type    = "DE425 DE425Adapter"
NetRuleHardwareDE425Class   = {"DE425Adapter basic"}
AdapterDE425Type   = 2  ;; EISA board
DE425CFID = 135185        ;; 0x00021011
DE425_1BYTE = 1346544400  ;;Compressed EISA ID "DEC4250"
EISA_MASK   = 4043309055


NetRuleHardwareBindForm = " yes yes container"
ProductKeyName  = $(!NTN_SoftwareBase)"\"$(Manufacturer)"\"$(ProductSoftwareName)"\CurrentVersion"
ParamKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)"\Parameters"

[GeneralConstants]
from        = ""
to          = ""
ExitCodeOk     = 0
ExitCodeCancel = 1
ExitCodeFatal  = 2
KeyNull           = ""
MAXIMUM_ALLOWED   = 33554432
RegistryErrorIndex = NO_ERROR
KeyProduct        = ""
KeyParameters   = ""
TRUE                = 1
FALSE             = 0
NoTitle                = 0
ExitState   = "Active"
OldVersionExisted = $(FALSE)
DriverPath        = $(!STF_NTPATH)\drivers
SystemsoftPresent = $(FALSE)
[date]
    Now = {} ? $(!LIBHANDLE) GetSystemDate

;---------------------------------------------------------------------------
; 1. Identify
;
; DESCRIPTION:   To verify that this INF deals with the same type of options
;                as we are choosing currently.
;
; INPUT:         None
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL
;                $($R1): Option Type (COMPUTER ...)
;                $($R2): Diskette description
;---------------------------------------------------------------------------

[Identify]
    read-syms Identification
    set Status     = STATUS_SUCCESSFUL
    set Identifier = $(OptionType)
    set Media        = #("Source Media Descriptions", 1, 1)
    Return $(Status) $(Identifier) $(Media)

;------------------------------------------------------------------------
; 2. ReturnOptions:
;
; DESCRIPTION:   To return the option list supported by this INF and the
;                localised text list representing the options.
;
;
; INPUT:         $($0):  Language used. ( ENG | FRN | ... )
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL |
;                                STATUS_NOLANGUAGE
;                                STATUS_FAILED
;                                STATUS_NOTSUPPORTED
;
;                $($R1): Option List
;                $($R2): Option Text List
;------------------------------------------------------------------------

[ReturnOptions]
    set Status          = STATUS_FAILED
    set OptionList     = {}
    set OptionTextList = {}
    ; check if language requested is supported
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) in $(LanguageList)
        ifstr(i) $($1) == ""
           goto returnoptions
        endif
        ; check if platform requested is supported
        set PlatformList = ^(PlatformsSupported, 1)
        Ifcontains(i) $($1) in $(PlatformList)
           goto returnoptions
        else
           set Status = STATUS_NOTSUPPORTED
           goto finish_ReturnOptions
        endif
    else
        set Status = STATUS_NOLANGUAGE
        goto finish_ReturnOptions
    endif
;form a list of all options and another of all the represnting text
returnoptions = +
    set OptionList     = ^(Options, 1)
    set OptionTextList = ^(OptionsText$($0), 1)
    set Status           = STATUS_SUCCESSFUL
finish_ReturnOptions = +
    Return $(Status) $(OptionList) $(OptionTextList)

;------------------------------------------------------------------------
;
; InstallOption:
;
;      This section is shelled to by main installation processing
;      or by NCPASHEL.INF during reconfig, removal, update, etc.
;
;
; FUNCTION:  To copy files representing Options
;            To configure the installed option
;            To update the registry for the installed option
;
; INPUT:     $($0):  Language to use
;            $($1):  OptionID to install
;            $($2):  SourceDirectory
;            $($3):  AddCopy  (YES | NO)
;            $($4):  DoCopy   (YES | NO)
;            $($5):  DoConfig (YES | NO)
;
; OUTPUT:    $($R0): STATUS: STATUS_SUCCESSFUL |
;                            STATUS_NOLANGUAGE |
;                            STATUS_USERCANCEL |
;                            STATUS_FAILED
;
;------------------------------------------------------------------------
[InstallOption]
    set Option   = $($1)
    set SrcDir   = $($2)
    set AddCopy  = $($3)
    set DoCopy   = $($4)
    set DoConfig = $($5)
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) NOT-IN $(LanguageList)
        Return STATUS_NOLANGUAGE
    endif
    set-subst LF = "\n"
    read-syms GeneralConstants
    read-syms FileConstants
    set NetRuleSoftwareBindable = $($R1)
    read-syms DialogConstants$(!STF_LANGUAGE)
    ifstr(i) $(!NTN_Origination) == "NCPA"
        set Continue = "OK"
    endif
    read-syms FileConstants$(!STF_LANGUAGE)
    detect date
    set-title  $(Function$(Option)Title)
    set to   = Begin
    set from = Begin
    set CommonStatus = STATUS_SUCCESSFUL
    EndWait
Begin = +
    Ifstr(i) $(!NTN_InstallMode) == deinstall
        set StartLabel = removeadapter
    else-Ifstr(i) $(!NTN_InstallMode) == Update
        set StartLabel = UpgradeSoftware
    else-Ifstr(i) $(!NTN_InstallMode) == bind
        set StartLabel = bindingadapter
    else-Ifstr(i) $(!NTN_InstallMode) == configure
          Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
                 Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_SOFTWARE
                 ifint $($ShellCode) != $(!SHELL_CODE_OK)
                     goto ShellCodeError
                 endif
                 set Error = $($R0)
                 set from = end
                 set to = end
                 goto nonfatalinfo
          else-ifstr(i) $(Option) == "DE425"
                 Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_HARDWARE
                 ifint $($ShellCode) != $(!SHELL_CODE_OK)
                     goto ShellCodeError
                 endif
                 set Error = $($R0)
                 set from = end
                 set to = end
                 goto nonfatalinfo
          else
                 set StartLabel = configureadapter
          endif
    else
        set StartLabel = installadapter
        set OEM_ABANDON_OPTIONS = {}
        set OEM_ABANDON_SOFTWARE = FALSE
        set OEM_ABANDON_ON = TRUE
    endif
    set from = $(fatal)
    set to = $(fatal)
    goto $(StartLabel)
installadapter = +
;--DEBUG -------------------------------------
        set !G:DebugOutputControl = $(ON)
;---------------------------------------------
;;for systemsoft cardwizard
    OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADBKeyName) $(MAXIMUM_ALLOWED) PCMCIADBKey
    ifstr $(PCMCIADBKey) == $(NULL)
        CloseRegKey $(PCMCIADBKey)
        Debug-Output "PCMCIA service not present"

    else
        OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADBKeyName)"\"$(DC21X4Manufacture) $(MAXIMUM_ALLOWED) PCMCIA$(DC21X4Manufacture)Key
        ifstr $(PCMCIA$(DC21X4Manufacture)Key) == $(NULL)
            debug-output "Adding "$(PCMCIADBKeyName)"\"$(DC21X4Manufacture)
            CreateRegKey $(PCMCIADBKey) {$(DC21X4Manufacture), 0, 0} "" $(MAXIMUM_ALLOWED) "" PCMCIA$(DC21X4Manufacture)Key
        else
            debug-output "Manufacture sub key already exist"
        endif
        OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADBKeyName)"\"$(DC21X4Manufacture)"\"$(DC21X4Model) $(MAXIMUM_ALLOWED) PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key
        ifstr $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) == $(NULL)
            debug-output "Adding "$(PCMCIADBKeyName)"\"$(DC21X4Manufacture)"\"$(DC21X4Model)
            CreateRegKey $(PCMCIA$(DC21X4Manufacture)Key) {$(DC21X4Model), 0, 0} "" $(MAXIMUM_ALLOWED) "" PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {Driver, 0, $(!REG_VT_SZ),$(ProductSoftwareName)}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {DeviceType,0,$(!REG_VT_SZ),"NET"}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {InfFileName,0,$(!REG_VT_SZ),$(STF_CONTEXTINFNAME)}
        else
            debug-output "Device sub key already exist"
            GetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key),+"Driver",GetData
            ifstr *($(GetData),7) != $(ProductSoftwareName)
              SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {Driver, 0, $(!REG_VT_SZ),$(ProductSoftwareName)}
              SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {DeviceType,0,$(!REG_VT_SZ),"NET"}
              SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {InfFileName,0,$(!REG_VT_SZ),$(STF_CONTEXTINFNAME)}
            endif
        endif
        CloseRegKey $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key)
        CloseRegKey $(PCMCIA$(DC21X4Manufacture)Key)
        CloseRegKey $(PCMCIADBKey)
      endif
      OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIARMPKeyName) $(MAXIMUM_ALLOWED) PCMCIARMKey
      ifstr $(PCMCIARMKey) == $(NULL)
        CloseRegKey $(PCMCIARMKey)
        Debug-Output "Systemsoft CardWizard service not present"
      else
        set SystemsoftPresent = $(TRUE)
        OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIARMKeyName) $(MAXIMUM_ALLOWED) PCMCIA$(DC21X4MacDB)Key
        ifstr $(PCMCIA$(DC21X4MacDB)Key) == $(NULL)
            debug-output "Adding "$(PCMCIARMKeyName)
            CreateRegKey $(PCMCIARMKey) {"MacDataBase" , 0, 0} "" $(MAXIMUM_ALLOWED) "" PCMCIA$(DC21X4MacDB)Key
            CloseRegKey PCMCIA$(DC21X4MacDB)Key
        endif
        CloseRegKey $(PCMCIARMKey)
      endif
        
;;this addition is for hot swap capability

    OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIARMKeyName) $(MAXIMUM_ALLOWED) PCMCIARMKey
    ifstr $(PCMCIARMKey) == $(NULL)
        CloseRegKey $(PCMCIARMKey)
        Debug-Output "Systemsoft CardWizard service not present"

    else
        OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIARMKeyName)"\"$(DC21X4Manufacture) $(MAXIMUM_ALLOWED) PCMCIA$(DC21X4Manufacture)Key
        ifstr $(PCMCIA$(DC21X4Manufacture)Key) == $(NULL)
            debug-output "Adding "$(PCMCIARMKeyName)"\"$(DC21X4Manufacture)
            CreateRegKey $(PCMCIARMKey) {$(DC21X4Manufacture), 0, 0} "" $(MAXIMUM_ALLOWED) "" PCMCIA$(DC21X4Manufacture)Key
        else
            debug-output "Manufacture sub key already exist"
        endif
        OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIARMKeyName)"\"$(DC21X4Manufacture)"\"$(DC21X4Model) $(MAXIMUM_ALLOWED) PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key
        ifstr $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) == $(NULL)
            debug-output "Adding "$(PCMCIARMKeyName)"\"$(DC21X4Manufacture)"\"$(DC21X4Model)
            CreateRegKey $(PCMCIA$(DC21X4Manufacture)Key) {$(DC21X4Model), 0, 0} "" $(MAXIMUM_ALLOWED) "" PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacDriverHandle, 0, $(!REG_VT_DWORD),0}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacDriverName,0,$(!REG_VT_SZ),$(ProductSoftwareName)}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacDriverState,0,$(!REG_VT_DWORD),1}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacDriverVersion,0,$(!REG_VT_DWORD),$(ProductMajorVersion)$(ProductMinorVersion)}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacSwapCapability,0,$(!REG_VT_DWORD),2}
        else
            debug-output "Device sub key already exist"
            GetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key),+"MacDriverName",GetData
            ifstr *($(GetData),7) != $(ProductSoftwareName)
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacDriverHandle, 0, $(!REG_VT_DWORD),0}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacDriverName,0,$(!REG_VT_SZ),$(ProductSoftwareName)}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacDriverState,0,$(!REG_VT_DWORD),1}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacDriverVersion,0,$(!REG_VT_DWORD),$(ProductMajorVersion)$(ProductMinorVersion)}
            SetRegValue $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key) {MacSwapCapability,0,$(!REG_VT_DWORD),2}
            endif
        endif
        CloseRegKey $(PCMCIA$(DC21X4Manufacture)$(DC21X4Model)Key)
        CloseRegKey $(PCMCIA$(DC21X4Manufacture)Key)
        CloseRegKey $(PCMCIARMKey)

    endif

;;;
;
;   First, check whether the same version of the software exists
;--------------------------------------------
; FOR DEBUGGING
; to debug the inf file change the OFF to ON
    set !G:DebugOutputControl = $(OFF)
; you will then be able to see debug prints of this kind:
    Debug-Output "oemsetup.inf: @#!$%"
;--------------------------------------------
    OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct
    Ifstr $(KeyProduct) != $(KeyNull)
        ; Same version already existed in the local machine
        ; Popup the dialog and ask the user whether he wants to continue
        CloseRegKey $(KeyProduct)
        ifstr(i) !(NTN_RegBase) == $(ProductKeyName)
           ;Cannot install the same software again
           Shell $(UtilityInf), VerExistedDlg, $(ProductSoftwareTitle),+
                 $(ProductVersion)
           ifint $($ShellCode) != $(!SHELL_CODE_OK)
                 goto ShellCodeError
           endif
           goto end
        else
           ; Add new adapter card?
           Shell $(UtilityInf), CardExistedDlg
           ifint $($ShellCode) != $(!SHELL_CODE_OK)
                goto ShellCodeError
           endif
           ifstr(i) $($R1) != "OK"
                 set CommonStatus = STATUS_USERCANCEL
                 goto end
           endif
           set OldVersionExisted = $(TRUE)
        endif
    Endif
    ifstr(i) $(DoCopy) == "YES"
        Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) YES
        Ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Goto ShellCodeError
        Else-Ifstr(i) $($R0) == STATUS_FAILED
            Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
            ifint $($ShellCode) != $(!SHELL_CODE_OK)
                 goto ShellCodeError
            endif
            set Error = $($R0)
                 Goto fatal
        Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
                 Goto successful
        Endif
        Set SrcDir = $($R1)
        install "Install-Hlp"
    endif
    Goto installproduct
configureadapter = +
    Ifstr(i) $(KeyProduct) == $(KeyNull)
        OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) $(MAXIMUM_ALLOWED) KeyProduct
        Ifstr $(KeyProduct) == $(KeyNull)
            Set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
           Goto fatalregistry
        Endif
    Endif
    Shell $(UtilityInf) FindService, $(KeyProduct)
    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Goto ShellCodeError
    Endif
    Ifstr(i) $($R0) != NO_ERROR
        Goto fatalregistry
    endif
    set KeyParameters = $($R2)
    CloseRegKey $($R1)
    Ifstr $(KeyParameters) == $(KeyNull)
        set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
        goto fatalregistry
    endif
    set OldVersionExisted = $(TRUE)
    set ValueName = ""
    set ValueData = ""
    set ValueStr  = ""
    set ValueList = {}
    ; Get the old values from the Registry      [Get Values]
    EnumRegValue $(KeyParameters) ValueList
    ForListDo $(ValueList)
        set ValueItem = $($)
        set ValueName = *($(ValueItem),1)
        set ValueData = *($(ValueItem),4)
        Ifstr(i) $(ValueName) == "ConnectionType"
            set ConnectionIndex = $(ValueData)
        endif
    EndForListDo
    set ConnectionValue = *($(ConnectionList), ~($(ConnectionValues),$(ConnectionIndex)))
    ifstr(i) $(ConnectionValue) == ""
        set ConnectionValue = *($(ConnectionList), 2)
    endif
adapteroptions = +
    ifstr(i) $(Option) != "DE425"
        set from = adapteroptions
        read-syms FileDependentDlg$(!STF_LANGUAGE)
        SetHelpFile $(!STF_WINDOWSSYSPATH)"\"$(OptionHelpFile) $(MinHelpId) $(MaxHelpId) $(Help$(Option)Id)
        ui start "InputDlg"
        ifstr(i) $(DLGEVENT) == "CONTINUE"
           set ConnectionIndex = $(Combo1Out)
           ui pop 1
        else-ifstr(i) $(DLGEVENT) == "BACK"
           set CommonStatus = STATUS_USERCANCEL
           ui pop 1
           goto end
        else
           ui pop 1
           goto end
        endif
        set ConnectionValue = *($(ConnectionValues), ~($(ConnectionList),$(ConnectionIndex)))
        ifstr(i) $(!NTN_InstallMode) == configure
           goto updateparameters
        endif
    endif
installproduct =+
    StartWait
    ifstr(i) $(Option) == "DE425"
        Shell $(UtilityInf), EISAFindBus, $($(Option)_1BYTE),$(EISA_MASK)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
             goto ShellCodeError
        endif
        ifstr $($R0) != "NO_ERROR"
             set Error = $($R0)
             goto fatal
        endif
        ifstr(i) $($R1) == {}
             set Error = $(CANNOT_FIND_ANY_CARD)
             set CommonStatus = USER_CANCEL
             set from = end
             goto nonfatal
        endif
        set AdapterList = $($R1)
    else
        set-div DeviceID = $($(Option)CFID) 65536
        Shell $(UtilityInf), GetPCIInformation, $(VendorID) $(DeviceID)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
             goto ShellCodeError
        endif
        ifstr(i) $($R0) == {}
             set Error = $(CANNOT_FIND_ANY_CARD)
             set CommonStatus = USER_CANCEL
             set from = end
             goto nonfatal
        endif
        set AdapterList = $($R0)
    endif
    ifint $(OldVersionExisted) == $(FALSE)
        Ifstr(i) $(DoCopy) == "YES"
           Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) YES
           Ifint $($ShellCode) != $(!SHELL_CODE_OK)
                 Goto ShellCodeError
           Else-Ifstr(i) $($R0) == STATUS_FAILED
                 Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
                 ifint $($ShellCode) != $(!SHELL_CODE_OK)
                  goto ShellCodeError
                 endif
                 set Error = $($R0)
                 Goto fatal
           Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
                 Goto successful
           Endif
           Set SrcDir = $($R1)
        Endif
        install "Install-Option"
        ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
           Shell $(UtilityInf) RegistryErrorString "UNABLE_COPY_FILE"
           ifint $($ShellCode) != $(!SHELL_CODE_OK)
                 goto ShellCodeError
           endif
           set Error = $($R0)
           goto fatal
        endif
        Shell $(UtilityInf), AddSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), +
            $(ProductSoftwareName), +
            $(ProductSoftwareTitle), $(STF_CONTEXTINFNAME), +
            $(ProductSoftwareImagePath), "kernel", "NDIS", {}, "",+
            $(NetEventDLL)
        Set OEM_ABANDON_SOFTWARE = TRUE
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif

        ;   At this point:
        ;     $R1 contains the product version key handle;
        ;     $R2 contains the NetRules subkey handle;
        ;     $R3 contains the new Services key handle;
        ;     $R4 contains the Parameters key
        ;     $R5 contains the Linkage Key

        set RegistryErrorIndex = $($R0)
        Ifstr(i) $(RegistryErrorIndex) != "NO_ERROR"
            EndWait
            CloseRegKey $($R1)
            CloseRegKey $($R2)
            CloseRegKey $($R3)
            CloseRegKey $($R4)
            CloseRegKey $($R5)
            goto fatalregistry
        endif
        Set SoftProductKey        = $($R1)
        Set SoftNetRuleKey        = $($R2)
        Set SoftServiceKey        = $($R3)
        Set SoftParameterKey    = $($R4)
        Set SoftLinkageKey        = $($R5)
        set NewValueList = {{SoftwareType,$(NoTitle),$(!REG_VT_SZ),$(SoftwareType)},+
                           {MajorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMajorVersion)},+
                           {MinorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMinorVersion)},+
                           {Title,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareTitle)},+
                           {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareDescription)},+
                           {ServiceName,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareName)},+
                           {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}
        Shell  $(UtilityInf), AddValueList, $(SoftProductKey), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set RegistryErrorIndex = $($R0)
        Ifstr(i) $(RegistryErrorIndex) != "NO_ERROR"
            EndWait
            CloseRegKey $(SoftProductKey)
            CloseRegKey $(SoftNetRuleKey)
            CloseRegKey $(SoftServiceKey)
            CloseRegKey $(SoftParameterKey)
            CloseRegKey $(SoftLinkageKey)
            goto fatalregistry
        endif
        set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareType)},+
                            {use,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareUse)}, +
                            {bindform,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareBindForm)}, +
                            {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareClass)}, +
                            {bindable,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareSWBindable)}, +
                            {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}
        Shell  $(UtilityInf), AddValueList, $(SoftNetRuleKey), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set RegistryErrorIndex = $($R0)
        CloseRegKey $(SoftProductKey)
        CloseRegKey $(SoftNetRuleKey)
        CloseRegKey $(SoftServiceKey)
        CloseRegKey $(SoftParameterKey)
        CloseRegKey $(SoftLinkageKey)
        Ifstr(i) $(RegistryErrorIndex) != "NO_ERROR"
            EndWait
            goto fatalregistry
        endif
    endif
    ForListDo $(AdapterList)
        set BusNum = *($($),1)
        set DeviceNum = *($($),2)
        set FunctionNum = *($($),3)
        ifstr(i) $(Option) == "DE425"
                Shell $(UtilityInf), IsNetCardAlreadyInstalled, $(BusNum), +
                    $(DeviceNum), $(ProductHardware$(Option)Description), $(ProductHardwareName) "YES"
                ifint $($ShellCode) != $(!SHELL_CODE_OK)
                    goto ShellCodeError
                endif
                ifstr $($R0) != "NO_ERROR"
                    set Error = $($R0)
                    goto fatal
                endif
                ifstr(i) $($R1) != "YES"
                        Shell $(UtilityInf), AddHardwareComponent, $(ProductHardwareName),$(STF_CONTEXTINFNAME),$(ProductKeyName)
                        ifint $($R4) != -1
                            Set OEM_ABANDON_OPTIONS = >($(OEM_ABANDON_OPTIONS), +
                                $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards\"$($R4))
                        endif
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                        set RegistryErrorIndex = $($R0)
                        Ifstr(i) $(RegistryErrorIndex) != "NO_ERROR"
                            EndWait
                            CloseRegKey $($R1)
                            CloseRegKey $($R2)
                            CloseRegKey $($R3)
                            goto fatalregistry
                        endif
                        Set HardNetCardKey        = $($R1)
                        Set HardNetRuleKey        = $($R2)
                        Set HardParameterKey    = $($R3)
                        set AdapterNumber = $($R4)
                        set NewValueList = {{Manufacturer,$(NoTitle),$(!REG_VT_SZ),$(Manufacturer)},+
                                           {Title,$(NoTitle),$(!REG_VT_SZ),"["$($R4)"] "$(ProductHardware$(Option)Title)},+
                                           {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductHardware$(Option)Description)},+
                                           {ProductName,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
                                           {ServiceName,$(NoTitle),$(!REG_VT_SZ),$($R5)},+
                                           {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}
                        Shell  $(UtilityInf), AddValueList, $(HardNetCardKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                        set BusTypeNum = 2
                        set NewValueList = {{AdapterType,$(NoTitle),$(!REG_VT_DWORD),$(Adapter$(Option)Type)},+
                                        {BusType,$(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
                                        {MediaType,$(NoTitle),$(!REG_VT_DWORD),1},+
                                        {BusNumber,$(NoTitle),$(!REG_VT_DWORD),$(BusNum)},+
                                        {SlotNumber,$(NoTitle),$(!REG_VT_DWORD),$(DeviceNum)},+
                                        {AdapterCFID,$(NoTitle),$(!REG_VT_DWORD),$($(Option)CFID)}}
                        Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                        set TempProdName = """"$(ProductHardwareName)$(AdapterNumber)""""
                        set TempBindForm = $(TempProdName)$(NetRuleHardwareBindForm)
                        set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleHardware$(Option)Type)},+
                                            {bindform,$(NoTitle),$(!REG_VT_SZ),$(TempBindForm)}, +
                                            {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleHardware$(Option)Class)}, +
                                            {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}
                        Shell  $(UtilityInf), AddValueList, $(HardNetRuleKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                        CloseRegKey $(HardNetCardKey)
                        CloseRegKey $(HardNetRuleKey)
                        CloseRegKey $(HardParameterKey)
                endif
        else
                Shell $(UtilityInf), IsNetCardAlreadyInstalled, $(BusNum), +
                    $(DeviceNum), $(ProductHardware$(Option)Description), $(ProductHardwareName) "YES"
                ifint $($ShellCode) != $(!SHELL_CODE_OK)
                    goto ShellCodeError
                endif
                ifstr $($R0) != "NO_ERROR"
                    set Error = $($R0)
                    goto fatal
                endif
                ifstr(i) $($R1) != "YES"
                  ifstr(i) $(!STF_GUI_UNATTENDED) != "YES"
                    read-syms FileDependentDlg$(!STF_LANGUAGE)
                    SetHelpFile $(!STF_WINDOWSSYSPATH)"\"$(OptionHelpFile) $(MinHelpId) $(MaxHelpId) $(Help$(Option)Id)
                    ui start "InputDlg"
                    ifstr(i) $(DLGEVENT) == "CONTINUE"
                         set ConnectionIndex = $(Combo1Out)
                         ui pop 1
                    else-ifstr(i) $(DLGEVENT) == "BACK"
                         set CommonStatus = STATUS_USERCANCEL
                         ui pop 1
                         goto end
                    else
                         ui pop 1
                         goto end
                    endif
                  endif
                    Shell $(UtilityInf), AddHardwareComponent, $(ProductHardwareName),$(STF_CONTEXTINFNAME),$(ProductKeyName)
                    ifint $($R4) != -1
                        Set OEM_ABANDON_OPTIONS = >($(OEM_ABANDON_OPTIONS), $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards\"$($R4))
                    endif
                    ifint $($ShellCode) != $(!SHELL_CODE_OK)
                        goto ShellCodeError
                    endif
                    set RegistryErrorIndex = $($R0)
                    Ifstr(i) $(RegistryErrorIndex) != "NO_ERROR"
                         EndWait
                         CloseRegKey $($R1)
                         CloseRegKey $($R2)
                         CloseRegKey $($R3)
                         goto fatalregistry
                    endif
                    set ConnectionValue = *($(ConnectionValues), ~($(ConnectionList),$(ConnectionIndex)))
                    ;   At this point:
                    ;     $R1  Registry key variable for HARDWARE\Netcard\(n)
                    ;     $R2  Registry key variable for HARDWARE\Netcard\(n)\\NetRules
                    ;     $R3  Registry key handle for <service>\Parameters key
                    ;     $R4  Adapter number assigned to adapter
                    ;     $R5  Service name generated by combining svc name with adapter number
                    Set HardNetCardKey        = $($R1)
                    Set HardNetRuleKey        = $($R2)
                    Set HardParameterKey    = $($R3)
                    set AdapterNumber = $($R4)
                    set NewValueList = {{Manufacturer,$(NoTitle),$(!REG_VT_SZ),$(Manufacturer)},+
                                        {Title,$(NoTitle),$(!REG_VT_SZ),"["$($R4)"] "$(ProductHardware$(Option)Title)},+
                                        {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductHardware$(Option)Description)},+
                                        {ProductName,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
                                        {ServiceName,$(NoTitle),$(!REG_VT_SZ),$($R5)},+
                                        {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}
                    Shell  $(UtilityInf), AddValueList, $(HardNetCardKey), $(NewValueList)
                    ifint $($ShellCode) != $(!SHELL_CODE_OK)
                         goto ShellCodeError
                    endif
                    set BusTypeNum = 5
                    ifint $(SystemsoftPresent) == $(TRUE)
                        set NewValueList = {{AdapterType,$(NoTitle),$(!REG_VT_DWORD),$(Adapter$(Option)Type)},+
                                           {MediaType,$(NoTitle),$(!REG_VT_DWORD),1},+
                                           {BusType,$(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
                                           {AdapterCFID,$(NoTitle),$(!REG_VT_DWORD),$($(Option)CFID)},+
                                           {PCMCIA,$(NoTitle),$(!REG_VT_DWORD),1}}
                    else
                        set NewValueList = {{AdapterType,$(NoTitle),$(!REG_VT_DWORD),$(Adapter$(Option)Type)},+
                                           {MediaType,$(NoTitle),$(!REG_VT_DWORD),1},+
                                           {BusType,$(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
                                           {AdapterCFID,$(NoTitle),$(!REG_VT_DWORD),$($(Option)CFID)}}
                    endif

                    Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                    ifint $($ShellCode) != $(!SHELL_CODE_OK)
                        goto ShellCodeError
                    endif
                    ifint $($(Option)CFID) == $(DC21041CFID)
                        set NewValueList = {{SnoozeMode,$(NoTitle),$(!REG_VT_DWORD),0}}
                        Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                        set NewValueList = {{NwayProtocol,$(NoTitle),$(!REG_VT_DWORD),1}}
                        Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                    endif
                    ifint $($(Option)CFID) == $(DC21142CFID)
                        set NewValueList = {{StoreAndForward,$(NoTitle),$(!REG_VT_DWORD),$(StoreAndForward)},+
                                            {SnoozeMode,$(NoTitle),$(!REG_VT_DWORD),0}}
                        Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                        set NewValueList = {{NwayProtocol,$(NoTitle),$(!REG_VT_DWORD),1}}
                        Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                    endif
                    ifint $($(Option)CFID) == $(DC21143CFID)
                        set NewValueList = {{StoreAndForward,$(NoTitle),$(!REG_VT_DWORD),$(StoreAndForward)},+
                                            {SnoozeMode,$(NoTitle),$(!REG_VT_DWORD),0}}
                        Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                    endif
                    ifint $($(Option)CFID) == $(DE450CFID)
                        set NewValueList = {{SnoozeMode,$(NoTitle),$(!REG_VT_DWORD),0}}
                        Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                    endif
                    ifint $($(Option)CFID) == $(DC21140CFID)
                        set NewValueList = {{StoreAndForward,$(NoTitle),$(!REG_VT_DWORD),$(StoreAndForward)},+
                                            {TransmitThreshold100,$(NoTitle),$(!REG_VT_DWORD),$(TxmThreshold100)},+
                                            {SnoozeMode,$(NoTitle),$(!REG_VT_DWORD),0}}
                        Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                    endif
                    ifstr(i) $(Option) == "MULTIA"
                        set NewValueList = {{ExternalSia,$(NoTitle),$(!REG_VT_DWORD),1},+
                                            {SiaRegister0,$(NoTitle),$(!REG_VT_DWORD),$(SiaRegister0)},+
                                            {SiaRegister1,$(NoTitle),$(!REG_VT_DWORD),$(SiaRegister1)},+
                                            {SiaRegister2,$(NoTitle),$(!REG_VT_DWORD),$(SiaRegister2)}}
                        Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                        ifint $($ShellCode) != $(!SHELL_CODE_OK)
                            goto ShellCodeError
                        endif
                    endif
                    set NewValueList = {{ConnectionType,$(NoTitle),$(!REG_VT_DWORD),$(ConnectionValue)}}
                    Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                    ifint $($ShellCode) != $(!SHELL_CODE_OK)
                        goto ShellCodeError
                    endif
                    set TempProdName = """"$(ProductHardwareName)$(AdapterNumber)""""
                    set TempBindForm = $(TempProdName)$(NetRuleHardwareBindForm)
                    set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleHardware$(Option)Type)},+
                                        {bindform,$(NoTitle),$(!REG_VT_SZ),$(TempBindForm)}, +
                                        {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleHardware$(Option)Class)}, +
                                        {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}
                    Shell  $(UtilityInf), AddValueList, $(HardNetRuleKey), $(NewValueList)
                    ifint $($ShellCode) != $(!SHELL_CODE_OK)
                        goto ShellCodeError
                    endif
                    CloseRegKey $(HardNetCardKey)
                    CloseRegKey $(HardNetRuleKey)
                    set NewValueList = {{BusNumber,$(NoTitle),$(!REG_VT_DWORD),$(BusNum)},+
                                        {SlotNumber,$(NoTitle),$(!REG_VT_DWORD),$(DeviceNum)},+
                                        {FunctionNumber,$(NoTitle),$(!REG_VT_DWORD),$(FunctionNum)}}
                    Shell  $(UtilityInf), AddValueList, $(HardParameterKey), $(NewValueList)
                    CloseRegKey $(HardParameterKey)
                endif
        endif
    EndForListDo
    ifstr(i) $(!STF_GUI_UNATTENDED) == "YES"
        Shell $(UtilityInf),AddDefaultNetCardParameters,$(KeyParameters)
    endif
    EndWait
    goto successful
updateparameters =+
    set HardParameterKey    = $($R3)
    set NewValueList = {{ConnectionType,$(NoTitle),$(!REG_VT_DWORD),$(ConnectionValue)}}
    Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    CloseRegKey $(KeyParameters)
    goto successful
bindingadapter =+
    set Error = "Binding: Sorry, not yet implemented."
    goto fatal
removeadapter = +
    Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
        Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set RegistryErrorIndex = $($R0)
        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    else
        Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), $(!NTN_RegBase)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set RegistryErrorIndex = $($R0)
        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    endif
    goto end
UpgradeSoftware = +
     OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct
     Ifstr $(KeyProduct) != $(KeyNull)
           Shell $(UtilityInf), GetInfFileNameFromRegistry, $(KeyProduct)
           ifint $($ShellCode) != $(!SHELL_CODE_OK)
                 Debug-Output "ShellCode error"
                 goto ShellCodeError
           endif
           set !UG_Filename = $($R0)
           install "Install-Update"
           ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
                 goto fatal
           endif
           SetRegValue $(KeyProduct) {MajorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMajorVersion)}
           SetRegValue $(KeyProduct) {MinorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMinorVersion)}
           CloseRegKey $(KeyProduct)
     else
           goto fatalregistry
     endif
     goto end
successful = +
    goto end
abandon = +
    ForListDo $(OEM_ABANDON_OPTIONS)
        Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), $($)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set RegistryErrorIndex = $($R0)
        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    EndForListDo
    Ifstr(i) $(OEM_ABANDON_SOFTWARE) == TRUE
        Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), FALSE
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set RegistryErrorIndex = $($R0)
        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    endif
    goto end
warning = +
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "WARNING", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
        goto $(to)
    else-ifstr(i) $($R1) == "CANCEL"
        goto $(from)
    else
        goto "end"
    endif
nonfatalinfo = +
    Set CommonStatus = STATUS_USERCANCEL
    Set Severity = STATUS
    goto nonfatalmsg
nonfatal = +
    Set Severity = NONFATAL
    goto nonfatalmsg
nonfatalmsg = +
    ifstr(i) $(Error) == ""
        Set Severity = NONFATAL
        Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), $(Severity), $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
        goto $(from)
    else
        goto "end"
    endif
fatalregistry = +
    Shell $(UtilityInf) RegistryErrorString $(RegistryErrorIndex)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    set Error = $($R0)
    goto fatal
fatal = +
    ifstr(i) $(Error) == ""
        Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "FATAL", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    goto setfailed
ShellCodeError = +
    set DlgType        = "MessageBox"
    set STF_MB_TITLE = $(ShellCodeErrorTitle)
    set STF_MB_TEXT  = $(ShellCodeErrorText)
    set STF_MB_TYPE  = 1
    set STF_MB_ICON  = 3
    set STF_MB_DEF   = 1
    ui start "Error Message"
    goto setfailed
setfailed = +
    set CommonStatus = STATUS_FAILED
    ifstr(i) $(OEM_ABANDON_ON) == TRUE
        set OEM_ABANDON_ON = FALSE
        goto abandon
    endif
    goto end
end = +
    goto term
term = +
    Return $(CommonStatus)
[Install-Option]
    set STF_VITAL = ""
    ifstr(i) $(AddCopy) == "YES"
        AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
    endif
    ifstr(i) $(DoCopy) == "YES"
         set !STF_NCPA_FLUSH_COPYLIST = TRUE
         CopyFilesInCopyList
    endif
    Exit
[Install-Hlp]
    set STF_VITAL = ""
    AddSectionFilesToCopyList Files-Hlp $(SrcDir) $(!STF_WINDOWSSYSPATH)
    set !STF_NCPA_FLUSH_COPYLIST = TRUE
    CopyFilesInCopyList
    Exit
[Install-Update]
    set STF_VITAL          = ""
    set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
    AddSectionFilesToCopyList Files-Hlp $(SrcDir) $(!STF_WINDOWSSYSPATH)
    AddSectionFilesToCopyList Files-Inf $(SrcDir) $(!STF_WINDOWSSYSPATH)
    AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
    set !STF_NCPA_FLUSH_COPYLIST = TRUE
    CopyFilesInCopyList
    exit
[Source Media Descriptions]
    1  = "Intel DC21x4 NDIS 4.0 Driver"
[ProductType]
STF_PRODUCT  = Winnt
STF_PLATFORM = I386
STF_PLATFORM = PPC
STF_PLATFORM = Alpha
[Files-Inf]
2,        oemsetup.inf,    SIZE=1000,     RENAME=$(!UG_Filename)
[Files-DC21040]
1,DC21X4.SYS , SIZE=999
[Files-DC21041]
1,DC21X4.SYS , SIZE=999
[Files-DC21140]
1,DC21X4.SYS , SIZE=999
[Files-DC21142]
1,DC21X4.SYS , SIZE=999
[Files-DC21143]
1,DC21X4.SYS , SIZE=999
[Files-EB40]
1,DC21X4.SYS , SIZE=999
[Files-EB41]
1,DC21X4.SYS , SIZE=999
[Files-EB140]
1,DC21X4.SYS , SIZE=999
[Files-EB142]
1,DC21X4.SYS , SIZE=999
[Files-EB143]
1,DC21X4.SYS , SIZE=999
[Files-E143DQS]
1,DC21X4.SYS , SIZE=999
[Files-MULTIA]
1,DC21X4.SYS , SIZE=999
[Files-DE434]
1,DC21X4.SYS , SIZE=999
[Files-DE435]
1,DC21X4.SYS , SIZE=999
[Files-DE450]
1,DC21X4.SYS , SIZE=999
[Files-DE500]
1,DC21X4.SYS , SIZE=999
[Files-DE425]
1,DC21X4.SYS , SIZE=999
[Files-Hlp]
1,DC21X4.HLP , SIZE=999
[LanguagesSupported]
    ENG
[OptionsTextENG]
    DC21040  = "Intel 21040 based Ethernet Controller"
    DC21041  = "Intel 21041 based Ethernet Controller"
    DC21140  = "Intel 21140 based 10/100 mpbs Ethernet Controller"
    DC21142  = "Intel 21142 based 10/100 mpbs Ethernet Controller"
    DC21143  = "Intel 21143 based 10/100 mpbs Ethernet Controller"
    EB40     = "Intel EB40 21040 based Evaluation board"
    EB41     = "Intel EB41 21041 based Evaluation board"
    EB140    = "Intel EB140 21140 based 10/100 mpbs Evaluation board"
    EB142    = "Intel EB142 21142 based 10/100 mpbs Evaluation board"
    EB143    = "Intel EB143 21143 based 10/100 mpbs Evaluation board"
    E143DQS  = "Intel EB143DQS 21143 based 10/100 mpbs only Evaluation board"
    MULTIA   = "DEC multia's Ethernet Controller"
    DE434    = "DEC DE434 EtherWORKS Turbo PCI TP Adapter"
    DE435    = "DEC DE435 EtherWORKS Turbo PCI Combo Adapter"
    DE450    = "DEC DE450 EtherWORKS Turbo PCI Combo Adapter"
    DE500    = "DEC DE500 FastEtherWORKS 10/100 PCI Adapter"
    DE425    = "DEC DE425 EtherWORKS Turbo EISA Adapter"
[FileConstantsENG]
ProCaption   = "Windows NT Setup"
ProCancel    = "Cancel"
ProCancelMsg = "Windows NT Networking is not correctly installed.  "+
                 "Are you sure you want to cancel copying files?"
ProCancelCap = "Network Setup Message"
ProText1     = "Copying:"
ProText2     = "To:"

ProductSoftwareDescription = "Intel DC21x4 Driver"

FunctionDC21040Title = "Intel 21040 based Ethernet Controller Setup"
ProductHardwareDC21040Description = "Intel 21040 based Ethernet Controller"

FunctionDC21041Title = "Intel 21041 based Ethernet Controller Setup"
ProductHardwareDC21041Description = "Intel 21041 based Ethernet Controller"

FunctionDC21140Title = "DIntel 21140 based 10/100 mpbs Ethernet Controller Setup"
ProductHardwareDC21140Description = "Intel 21140 based 10/100 mpbs Ethernet Controller"

FunctionDC21142Title = "Intel 21142 based 10/100 mpbs Ethernet Controller Setup"
ProductHardwareDC21142Description = "Intel 21142 based 10/100 mpbs Ethernet Controller"

FunctionDC21143Title = "Intel 21143 based 10/100 mpbs Ethernet Controller Setup"
ProductHardwareDC21143Description = "Intel 21143 based 10/100 mpbs Ethernet Controller"

FunctionEB40Title    = "Intel EB40 21040 based Evaluation Board Setup"
ProductHardwareEB40Description    = "Intel EB40 21040 based Board"

FunctionEB41Title    = "Intel EB41 21041 based Evaluation Board Setup"
ProductHardwareEB41Description    = "Intel EB41 21041 based Evaluation Board"

FunctionEB140Title    = "Intel EB140 21140 based 10/100 mpbs Evaluation Board Setup"
ProductHardwareEB140Description    = "Intel EB140 21140 based Evaluation Board"

FunctionEB142Title    = "Intel EB142 21142 based 10/100 mpbs Evaluation Board Setup"
ProductHardwareEB142Description    = "Intel EB142 21142 based Evaluation Board"

FunctionEB143Title    = "Intel EB143 21143 based 10/100 mpbs Evaluation Board Setup"
ProductHardwareEB143Description    = "Intel EB143 21143 based Evaluation Board"

FunctionE143DQSTitle    = "Intel EB143DQS_20 21143 based 10/100 mpbs only Evaluation Board Setup"
ProductHardwareE143DQSDescription    = "Intel E143DQS 21143 based Evaluation Board"


FunctionMULTIATitle = "DEC multia's Ethernet Controller Setup"
ProductHardwareMULTIADescription = "DEC multia's Ethernet Controller"

FunctionDE434Title   = "DEC DE434 PCI Adapter Card Setup"
ProductHardwareDE434Description   = "DEC DE434 EtherWORKS Turbo PCI TP Adapter"

FunctionDE435Title   = "DEC DE435 PCI Adapter Card Setup"
ProductHardwareDE435Description   = "DEC DE435 EtherWORKS Turbo PCI Combo Adapter"


FunctionDE450Title   = "DEC DE450 PCI Adapter Card Setup"
ProductHardwareDE450Description   = "DEC DE450 EtherWORKS Turbo PCI Combo Adapter"

FunctionDE500Title   = "DEC DE500 PCI Adapter Card Setup"
ProductHardwareDE500Description   = "DEC DE500 FastEtherWORKS 10/100 PCI Adapter"

FunctionDE425Title   = "DEC DE425 EISA Adapter Card Setup"
ProductHardwareDE425Description   = "DEC DE425 EtherWORKS Turbo EISA Adapter"

ConnectionList  = ^(ConnectionChoices$(Option), 1)
ConnectionValues = ^(ConnectionChoices$(Option), 2)
NoList  = ^(NoChoices, 1)
NoValues = ^(NoChoices, 2)
ShellCodeErrorTitle     = "Error: "$(Function$(Option)Title)
ShellCodeErrorText        = "Shell Code Error."
CANNOT_FIND_ANY_CARD    = "Network card is not present in the system"
[DialogConstantsENG]
Help          = "&Help"
Exit          = "Cancel"
OK            = "OK"
HelpContext = ""
Continue    = "Continue"
Cancel        = "Cancel"

[FileDependentDlgENG]
DlgText = "Choose the proper cable type for the "+
          "network adapter. Select [Help] for a detailled "+
          "description of the available options of the list."
DlgTemplate = "ADAP_PROTO_COMBO"
DlgType = "Combination"
Caption = $(Function$(Option)Title)
Combo1Label = "&Connection Type:"
Combo1List = $(ConnectionList)
Combo1Out  = $(ConnectionValue)
ComboListItemsIn  = {Combo1List}
ComboListItemsOut = {Combo1Out}
EditTextLim = ""
CBOptionsGreyed = {}
MinHelpId = 10
MaxHelpId = 1140
HelpContext = $(Help$(Option)Id)

